The RFB server implementation is still lacking as of now, as a consequence
you should force 8bit mode on the client to use it correctly, i.e. on Linux,
use: "xvncviewer -bgr233 localhost" or similar.
