----------------------
  CPU-Z version 1.31
----------------------

CPUID Output
------------------------------------------------------------------------------

Number of CPUs			1
Name				Intel Pentium II
Code name			Klamath
Specification			Intel Pentium II 300 MHz
Family/Model/Stepping		634
Extended Family/Model		0/0
Package				Slot 1 SECC
Core Stepping			C1
Technology			0.35µ
Instructions Sets		MMX
Features			
Clock Speed			299.1 MHz
Clock multiplier		x4.5
Front Side Bus Frequency	66.5 MHz
Bus Speed			66.5 MHz
Stock frequency			300 MHz
L1 Data Cache			16 KBytes, 4-way set associative, 32 Bytes line size
L1 Instruction Cache		16 KBytes, 4-way set associative, 32 Bytes line size
L2 Cache			512 KBytes, 4-way set associative, 32 Bytes line size
L2 Latency			0
L2 Speed			149.6 MHz (1/2)
L2 Location			On Cartridge
L2 ECC Check			enabled
L2 Data Prefetch Logic		no
L2 Bus Width			64 bits

				eax		ebx		ecx		edx
Function 00000000		00000002	756e6547	6c65746e	49656e69
Function 00000001		00000634	00000000	00000000	0080fbff
Function 00000002		03020101	00000000	00000000	0c040843

				edx		eax
MSR 0000002A			00000000	C5800000
MSR 0000011E			00000000	00044521
MSR 0000008B			00000037	00000000
